{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":6,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Léc hossza (cm)",92]
[null,"Léc tömege (gramm)",178]
[null,"1 méter léc tömege (gramm)",{"$f":"C10*100/C9","v":193.47826086956522}]
[null,"Kamera tömege (gramm)",236]
[null,"Kamera a léc végétől (cm)",3]
[null,"Ellensúly (gramm)",1000]
[null,"Becsült alátámasztás (cm)",20.644978783592641]
[]
[null,"Nyomatékegyensúly",{"$f":"alátámasztás/100*métersúly*alátámasztás/2+ellensúly*alátámasztás-(hossz-alátámasztás)/100*métersúly*(hossz-alátámasztás)/2-kamera*(hossz-alátámasztás-kamerapont)","v":0}]
[]
[]
[]
[null,null,null,null,"www.heatwave.hu"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}